Katelin Kaneen

Southern New Hampshire University

CS-350-X6152 Emerging Sys Arch & Technology

July 16, 2023

1. How does the Macro UART\_DATA\_BINARY impacts the UART?

Macro of UART\_DATA\_BINARY impacts UART by reading the data but not processed.

1. How does the Macro UART\_RETURN\_FULL impact the UART?

UART\_RETURN\_FULL means that it will process or read when the buffer has been filled

1. What driver call would you use to write 10 characters out of the UART?  
   UART\_Write is a function that will to write 10 characters out of UART
2. What is the driver call to turn off LED 0?

The driver within my code that turns off LED 0 is GPIO\_write(CONFIG\_GPIO\_LED\_0, CONFIG\_GPIO\_LED\_OFF);

1. What is the UART baud rate?

The uartParams.baudRate = 115200 within the uartecho.c.